Moving roads

This Chapter deals with moving roads only. Roads without cars have different rules and are described in another chapter.

These moving roads can be easily used almost like static roads of fixed height as there is no extended operation of cars like that of trains over the end points. The difficulty is two fold: These macros affect scenery buffer and frame rate more than the rails and they are rather long, typically a multiple of 800 m. Buffer considerations make the use of very long pieces mandatory for FS98 and reduces the number of possible macros to very few for FS95. This may make it difficult to place them, other than on very long bridges, into scenery with dense railways. My recommendation therefore is that you lay the roads first (planning where the bridges are expected to cross over rails), the moving railways second, the static railways third, and other 3D-objects last.

The cars that move are defined in a car list. The cars run at 60 km/h. The traffic is repeated every 8 slots.

As usual the strategy for bridges has to be different for FS95/98 and FS2000.

The following moving roads are available:

M8Ro0600 | Length 800m
M8Ro0800 | Length 800m
M8Ro1000 | Length 16000m
M8Ro1100 | Length 1100m
M8Ro1200 | Length 1200m
M8Ro1600 | Length 1600m
M8Ro2400 | Length 2400m
M8Ro3200 | Length 3200m
M8Ro4000 | Length 4000m
M8Ro4800 | Length 4800m
M8RC10 | Curved 10 degrees, 3 x 800m
M8RC20 | Curved 20 degrees, 3 x 800m
M8RC40 | Curved 40 degrees, 5 x 800m
M8RB0800 | Small road bridge 800m for FS95/98/2000 to cross a small river, road, or rail.
M8RX0800 | Two moving roads crossing asymmetrical. Secured by signal lights.
| FS2000 only:
M8RBi800 | 800m bridge for FS2000 only.
M8Rc0458 | 456m ramp climbing 4m.
M8Rc0800 | 800m ramp climbing 7m.
M8RR0458 | 458m ramp climbing 8m.
M8RR0800 | 800m ramp climbing 14m.
M8RR1600 | 1600m ramp climbing 28m.
M8RRx800 | 800m ramp climbing 28m.

All moving roads are called with the same parameters:

Parameter | Value | Meaning
%1 |  | Geographical width
%2 |  | Geographical Length
%3 | 0 | Road is placed on the surface of the FS terrain.
| Unequal 0 | Absolute altitude of the road above sea level in m
%4 | 0.250 | Scale. Should always be 0.250.
%5 | Orientation | Orientation of the road on the terrain (0 = south-north direction)
%6 | 0-10 | Two digit number. First digit >= 1 switches on lamps and night illumination Second digit switches on a line of bushes or trees with height of second digits.
%7 |  | Car list 1 - 9
%8 |  | Car list of the second road on a cross Bridge rail for bridges
%9 | 0-105 | Embankment color 0: No embankment 1-FF: FS color 100-104: Texture 105: Seasonal texture
%10 |  | Range in m Road is visible if within range. Typical value is 7000. The last digit is used to encode the road texture.

Hints:

You can modify the sequence of cars by editing the files ..\includes\rolistn.inc. The current implementation of cars is optimized for size, not for frame rate, to allow their use in FS98. This may change in a future version when usage in FS98 is no longer needed and multi-megabytes of free memory are available in system and video RAMs.