#### This is a big straight bridge for single to quad rail, 50 to 800 m long, crossing nothing at a variable height. It is intended for a railway to cross rivers, FS-roads and other 2-dimensional objects, or three dimensional objects in FS2000. The bases of the pylons are very tall to cross deep valleys. The bridge supports trains and power lines. The bridge rails can be varied. Do not use these bridges with FS95 or FS98.

Available macros are:

Length\Width | Single | Dual | Triple | Quad
050 m* | Brid1050 | Brid2050 | Brid3050 | Brid4050
100m * | Brid1100 | Brid2100 | Brid3100 | Brid4100
200m * | Brid1200 | Brid2200 | Brid3200 | Brid4200
300m + | Brid1300 | Brid2300 | Brid3300 | Brid4300
400m + | Brid1400 | Brid2400 | Brid3400 | Brid4400
500m + | Brid1500 | Brid2500 | Brid3500 | Brid4500
600m + | Brid1600 | Brid2600 | Brid3600 | Brid4600
800m * | Brid1800 | Brid2800 | Brid3800 | Brid4800

- * Only callable as user defined rails.
- + You call these rails instead of the FS95/98 ones by checking the appropriate box:

The following parameters are used:

Airport Name | SCASM | Meaning
Height | %3 | The height above ground in m. This is 0 for 2D-designs and has to be set for 3D-Designs to 0.01 minimum.
Scale | %4 | Scale, should always be 0.25 (for German systems 0,25 )
Heading | %5 | Deviation from the south/north axis in degrees So 90 means west/east
Parameter 0 | %6 | Electrical Power lines for the rail 0 = No power 1 = Wires only 2 = Simple pylons and wires 3 = Textured pylons and wires 4 = Textured pylons and wires and lamps
Parameter 1 | %7 | Train#. All trains are possible but I recommend only trains of a maxumum of 200m due to the outer parts having a slight slope.
Parameter 2 | %8 | Height of the bridge in units of 0.25 m
Parameter 3 | %9 | Word describing details, 3 variables abc a is used for the lower part: a >= 1 a lower side is drawn a >= 2 the middle pylon is placed b (0 – 6) describes the shape of the bridge rail, 0 means no bridge rail as in example 1-6 below. c ( 0 – 9) chooses the color
Visibility | %10 | Visibility range.