Bridges for rails crossings rails

Bridges of this type have many things in common. The upper rail at height 28 (7 m) runs from west to east and has a length of 50m. It can be of 6 types: single, dual, triple, quad rail, road or highway. The rail can be electrified with a central simple or textured pylon. The lower rail of 50m length can be a single to quad rail and can be electrified. All combinations exist for an angle of 90 degrees between the two rails. The complete edition will have many macros with different angles (30, 45, 60, 75, 90, 105, 120, 135, 150) degrees. The lower rail is one unit = 25 cm height.

The opening of these bridges is wide enough to allow a road or a small river to run parallel to the bridge. The name of the macros is Bridgelh.api, where l = (1, 2, 3, 4) describes the type of the lower rail and h = (1, 2, 3, 4, s, h) describes the upper rail, road or highway. The bridges with other angles are Bridgalh.api (30 degrees), Bridgb... .

AIRPORT parameter 2 ( %8) fixes the shape of the bridge rail. There are 4 forms and 8 colors available. The embankment for the upper rail can be chosen in the usual way.
Available bridges are:

Lower rail Upper Rail | Single | Dual | Triple | Quadruple
Single | Bridge11.api | Bridge21.api | Bridge31.api | Bridge41.api
Dual | Bridge12.api | Bridge22.api | Bridge32.api | Bridge42.api
Triple | Bridge13.api | Bridge23.api | Bridge33.api | Bridge43.api
Quadruple | Bridge14.api | Bridge24.api | Bridge34.api | Bridge44.api
Road | Bridge1s.api | Bridge2s.api | Bridge3s.api | Bridge4s.api
Highway | Bridge1h.api | Bridge2h.api | Bridge3h.api | Bridge4h.api

These bridges are the only proper way to lead a static railway over another static railway in FS95 and FS98. With FS2000 you can easily use the set of bridges Bridnlll to cross any ground rail.

The calling sequence is:

Airport Name | SCASM | Meaning
Scale | %4 | Scale, should always be 0.25 (for German systems 0,25 )
Heading | %5 | Deviation from the south/north axis in degrees So 90 means west/east
Parameter 0 | %6 | Electrical Power lines for the lower rail 0 = No power 1 = Wires only 2 = Simple pylons and wires 3 = Textured pylons and wires
Parameter 1 | %7 | Electrical Power lines for the upper rail 0 = No power 1 = Wires only 2 = Simple pylons and wires 3 = Textured pylons and wires
Parameter 2 | %8 | Shape of the bridge rails. Decimal number 0 = no bridge rail nm = shape n color m, n = 0…3, m = 1…8 n=0 n=1 n=2 n=3 nm >= 40 a small wall, 75cm high, with color %8-40.
Parameter 3 | %9 | Color scheme for the embankment Hexadecimal number 0 = no embankment drawn 1-FF = FS color. 100 Textured embankment with grass.r8 101 Textured embankment with broads.r8 102 Textured embankment with bushmnt.r8 intended for users of MOUNTAIN by Hans Meier 103 Textured embankment with desert.r8 104 Textured embankment with arid.r8 Please contact me if you want to propose additional textures
Visibility | %10 | Visibility range.