#### This is a big straight bridge for single to quad rail, 300 to 600 m long, crossing nothing at a variable height. It is intended for a railway to cross rivers, FS-roads, the roads in HDDS© technology, some special HDDS© rails, smaller valleys, and other 2-dimensional objects. The bridge supports trains and power lines. The bridge rails can be varied. The following example is called with (3,-602,28,221).

Available macros are:

Length\Width | Single | Dual | Triple | Quad
300 m | Bri1300 | Bri2300 | Bri3300 | Bri4300
400 m | Bri1400 | Bri2400 | Bri3400 | Bri4400
500 m | Bri1500 | Bri2500 | Bri3500 | Bri4500
600 m | Bri1600 | Bri2600 | Bri3600 | Bri4600

The following parameters are used:

Airport Name | SCASM | Meaning
Scale | %4 | Scale, should always be 0.25 (for German systems 0,25 )
Heading | %5 | Deviation from the south/north axis in degrees So 90 means west/east
Parameter 0 | %6 | Electrical Power lines for the rail 0 = No power 1 = Wires only 2 = Simple pylons and wires 3 = Textured pylons and wires 4 = Textured pylons and wires and lamps
Parameter 1 | %7 | Train#. All trains are possible but I recommend using only trains of a maximum of 200m due to the outer parts having a slight slope.
Parameter 2 | %8 | Height of the bridge in units of 0.25 m. If a rail bridge like bridge22.api is directly attached this has to be 28.
Parameter 3 | %9 | Word describing details with 3 variables abc a is used for the lower part: a >= 1 a lower side is drawn a >= 2 the middle pylon is placed b (0 – 6) describes the shape of the bridge rail, 0 means no bridge rail as in example 1-6 below. c (0 – 9) chooses the color
Visibility | %10 | Visibility range.